; OEMSETUP.INF

[Version]
Signature="$CHICAGO$"
Class=Printer
Provider=%GRAPHTEC%

[Manufacturer]
%GRAPHTEC%           =Mfg.Graphtec

[Mfg.Graphtec]
"Graphtec GX3000"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec MP5000"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FP8000"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FP9000"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec PT-5M"                  = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec CE1000-60"              = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec CE2000-60/2000-120"     = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec CE2000-120AP"           = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FC2230"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FC3200-50"              = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FC4100"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FC4200"                 = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec FC5100"                 = GRAPHTEC_USB.DRV,USB\GraphtecFC510057E8
"Graphtec TM1030/1130"            = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1040/1140/1240"       = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1031/1131"            = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1220/1300(STD)"       = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1220/1300(BINARY)"    = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1220/1300(SOLID)"     = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec TM1220/1300(RASTER)"    = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec JC9000/9100"            = GRAPHTEC_COLOR80.DRV,Graphtec_Plotter
"Graphtec JX1130/1060"            = GRAPHTEC.DRV,Graphtec_Plotter
"Graphtec JX2100/2150"            = GRAPHTEC_JX20.DRV,Graphtec_Plotter

[GRAPHTEC.DRV]
CopyFiles=GRAPHTEC
DataSection=GRAPHTEC_DATA

[GRAPHTEC_USB.DRV]
CopyFiles=GRAPHTEC,MONITOR
DataSection=GRAPHTEC_DATA
PortMonitor=%PortMon%

[GRAPHTEC_COLOR80.DRV]
CopyFiles=GRAPHTEC,COLOR_TABLE80
DataSection=GRAPHTEC_DATA

[GRAPHTEC_JX20.DRV]
CopyFiles=GRAPHTEC,COLOR_TABLEJX
DataSection=GRAPHTEC_DATA

[GRAPHTEC]
GRAPHTEC.DRV,GRAPHTEC.DR_
GRAPHTEC.HLP

[MONITOR]
GTCUPMON.DLL,GTCUPMON.DL_

[COLOR_TABLE80]
JC80AXPM.TBC,JC80AXPM.TB_
JC80AXST.TBC,JC80AXST.TB_
JC80AXTC.TBC,JC80AXTC.TB_
JC80AXTM.TBC,JC80AXTM.TB_
JC80JRPF.TBC,JC80JRPF.TB_
JC80PRG.TBC,JC80PRG.TB_
JC80RVLM.TBC,JC80RVLM.TB_

[COLOR_TABLEJX]
PRG.JX2,PRG.JX_

[GRAPHTEC_DATA]
NoTestPage=1
DriverFile=GRAPHTEC.DRV
DataFile=GRAPHTEC.DRV
HelpFile=GRAPHTEC.HLP
DefaultDataType=EMF
RetryTimeout=600
NotSelectedTimeout=600

[DestinationDirs]
DefaultDestDir=11
COLOR_TABLE80=23
COLOR_TABLEJX=23

[SourceDisksFiles]
GRAPHTEC.DR_ = 1
JC80AXPM.TB_ = 1,..\Color
JC80AXST.TB_ = 1,..\Color
JC80AXTC.TB_ = 1,..\Color
JC80AXTM.TB_ = 1,..\Color
JC80JRPF.TB_ = 1,..\Color
JC80PRG.TB_ = 1,..\Color
JC80RVLM.TB_ = 1,..\Color
PRG.JX_ = 1,..\Color
GTCUPMON.DL_ = 1

[SourceDisksNames]
1="OPS628 Windows Plotter Driver",,0

[Strings]
Graphtec="Graphtec"
PortMon="GTCUPMON,GTCUPMON.DLL"
