How to update the MPC6525A firmware version to V4315
(1)  Copy the two files 6525A4315.2AF and 6525A4311.2AH to the root of a USB Mass Storage Device. It's better to remove any other files from the device.
(2)  Power off the control board.
(3)  Insert the USB Mass Storage Device into the board.
(4)  Power on the control board
(5)  You do not remove the USB Mass Storage Device for about 1 minute.
(6)  Remove the USB Mass Storage Device from the control board.

How to update the MPC6525A DLL version to V4308
Copy mpc05ls.dll file to replace old one in your installed directory.

The firmware V4315 is compatible with the DLL V4308.

June 2013
Leetro Automation Co., Ltd.
overseas@leetro.com
==============================================================================================================================================
