Graphtec Plotter Driver OPS628 Ver. 7.12
for Microsoft Windows 95 / 98 / Me / Windows NT 4.0 / Windows 2000 / Windows XP

Thank you for choosing the Graphtec OPS628 Plotter Driver. 

The README.TXT file in each directory contains instructions on installation and
operation as well as other notes. Be sure to read them carefully before 
installing or using this driver.

Before you begin installation, check that the program disk contains the 
following:
  WIN9X_ME\GRAPHTEC.DR_     For Windows 95/98/Me
  WIN9X_ME\GRAPHTEC.HLP
  WIN9X_ME\GTCUPMON.DL_
  WIN9X_ME\GTCUSBP.SY_
  WIN9X_ME\OEMSETUP.INF
  WIN9X_ME\USBPRINT.INF
  WIN9X_ME\README.TXT

  WINNT40\DISK1             For Windows NT4.0
  WINNT40\GPGL.DL_
  WINNT40\GPGLUI.DL_
  WINNT40\GPGLUI.HLP
  WINNT40\OEMSETUP.INF
  WINNT40\README.TXT
  WINNT40\GX3000.GPD
  WINNT40\MP5000.GPD
  WINNT40\FP8000.GPD
  WINNT40\FP9000.GPD
  WINNT40\PT5M.GPD
  WINNT40\CE1000.GPD
  WINNT40\CE2000.GPD
  WINNT40\CE2120AP.GPD
  WINNT40\FC2230.GPD
  WINNT40\FC3200.GPD
  WINNT40\FC4100.GPD
  WINNT40\FC4200.GPD
  WINNT40\FC5100.GPD
  WINNT40\TM1040.GPD
  WINNT40\TM1030.GPD
  WINNT40\TM1031.GPD
  WINNT40\TM1220.GPD
  WINNT40\TM1220B.GPD
  WINNT40\TM1220S.GPD
  WINNT40\TM1220R.GPD
  WINNT40\JC9000.GPD
  WINNT40\JX1000.GPD
  WINNT40\JX2000.GPD

  WIN2K_XP\DISK1             For Windows 2000 / Windows XP
  WIN2K_XP\OEMSETUP.INF
  WIN2K_XP\README.TXT
  WIN2K_XP\GX3000.GPD
  WIN2K_XP\MP5000.GPD
  WIN2K_XP\FP8000.GPD
  WIN2K_XP\FP9000.GPD
  WIN2K_XP\PT5M.GPD
  WIN2K_XP\CE1000.GPD
  WIN2K_XP\CE2000.GPD
  WIN2K_XP\CE2120AP.GPD
  WIN2K_XP\FC2230.GPD
  WIN2K_XP\FC3200.GPD
  WIN2K_XP\FC4100.GPD
  WIN2K_XP\FC4200.GPD
  WIN2K_XP\FC5100.GPD
  WIN2K_XP\TM1040.GPD
  WIN2K_XP\TM1030.GPD
  WIN2K_XP\TM1031.GPD
  WIN2K_XP\TM1220.GPD
  WIN2K_XP\TM1220B.GPD
  WIN2K_XP\TM1220S.GPD
  WIN2K_XP\TM1220R.GPD
  WIN2K_XP\JC9000.GPD
  WIN2K_XP\JX1000.GPD
  WIN2K_XP\JX2000.GPD
  WIN2K_XP\GTCGLMON.DL_

  COLOR\JC80AXPM.TB_        For Color Adjustment
  COLOR\JC80AXST.TB_
  COLOR\JC80AXTC.TB_
  COLOR\JC80AXTM.TB_
  COLOR\JC80JRPF.TB_
  COLOR\JC80PRG.TB_
  COLOR\JC80RVLM.TB_
  COLOR\PRG.JX_

Precautions to be observed when connecting the FC5100 via USB
  * Supported OS
      Windows 98/Me, Windows 2000 Professional, or Windows XP
  * The plotter does not operate under Windows 3.1/95 or Windows NT.
  * Operation with other than the included driver is not guaranteed.
  * Do not connect multiple plotters to a single computer.
  * Operation is not guaranteed if the plotter is connected to a USB hub or to 
    a USB extension board. 

END
